===== Config file =====
[gcode_macro CALIBRATE_NOZZLE_OFFSET]
description = Move to center of bed and calibrate nozzle offset
gcode = 
	G90
	G0 X100 Y155 F1500
	PROBE_CALIBRATE

[gcode_macro LEVEL_BED]
description = "Level the bed manually."
gcode = 
	BED_SCREWS_ADJUST

[gcode_macro CHECK_DEVIATION]
description = "Check the deviation of the bed from the last loaded mesh."
gcode = 
	SCREWS_TILT_CALCULATE MAX_DEVIATION=0.05

[gcode_macro LIZ_IS_A_BAKA]
description = "Liz is a baka, so here's her start G-Code >.<"
gcode = 
	BED_MESH_CALIBRATE
	BED_MESH_PROFILE SAVE=default

[gcode_macro _START_GCODE]
description = "The gcode that should be called from your slicer at the beginning of a print."
gcode = 
	
	G90
	G1 X2 Y30 Z30 F1500
	G1 Z0.28 F240
	G92 E0
	G1 Y220 E10 F1500
	G1 X2.3 F5000
	G92 E0
	G1 Y30 E10 F1200
	G92 E0
	G1 Z5 F1500

[gcode_macro _END_GCODE]
description = "The gcode that should be called from your slicer at the end of a print."
gcode = 
	G91
	G1 E-2 F2700
	G1 E-2 Z0.2 F2400
	G1 X5 Y5 F3000
	G1 Z10
	G90
	
	G1 X0 Y220
	M106 S0
	M104 S0
	M140 S0
	
	M84 X Y E

[stepper_x]
step_pin = PC0
dir_pin = PL1
enable_pin = !PA7
microsteps = 16
rotation_distance = 33
endstop_pin = ^!PB6
position_endstop = 0
position_max = 298
homing_speed = 50

[stepper_y]
step_pin = PC1
dir_pin = !PL0
enable_pin = !PA6
microsteps = 16
rotation_distance = 46
endstop_pin = ^!PB5
position_endstop = 0
position_max = 280
homing_speed = 50

[stepper_z]
step_pin = PC2
dir_pin = PL2
enable_pin = !PA5
microsteps = 16
rotation_distance = 8
endstop_pin = probe:z_virtual_endstop
position_max = 250

[bltouch]
sensor_pin = ^PB4
control_pin = PL5
x_offset = -44
y_offset = 8
z_offset = 2.850

[bed_mesh]
speed = 120
horizontal_move_z = 7
mesh_min = 30, 40
mesh_max = 250, 230
probe_count = 5
mesh_pps = 3
algorithm = bicubic

[safe_z_home]
home_xy_position = 140, 140
speed = 50
z_hop = 10
z_hop_speed = 5

[extruder]
step_pin = PC3
dir_pin = PL6
enable_pin = !PA4
microsteps = 16
rotation_distance = 7.9797
nozzle_diameter = 0.400
heater_pin = PH6
filament_diameter = 1.750
sensor_type = NTC 100K MGB18-104F39050L32
sensor_pin = PF0
min_temp = 0
max_temp = 990
control = pid
pid_kp = 23.769
pid_ki = 1.248
pid_kd = 113.201

[heater_bed]
heater_pin = PE5
sensor_type = EPCOS 100K B57560G104F
sensor_pin = PF2
control = watermark
min_temp = 0
max_temp = 130
max_power = 1.0

[verify_heater heater_bed]
heating_gain = 1
check_gain_time = 60

[fan]
pin = PH3

[heater_fan heatbreak_cooling_fan]
pin = PH5
fan_speed = 1.0
heater = extruder
heater_temp = 50.0

[mcu]
serial = /dev/serial/by-id/usb-UltiMachine__ultimachine.com__RAMBo_6403335373035101E171-if00
baud = 250000

[printer]
kinematics = cartesian
max_velocity = 300
max_accel = 3000
max_z_velocity = 5
max_z_accel = 100

[ad5206 stepper_digipot]
enable_pin = PD7
scale = 2.08
channel_1 = 1.34
channel_2 = 1.0
channel_4 = 1.1
channel_5 = 1.1
channel_6 = 1.1

[static_digital_output stepper_config]
pins = 
	PG1, PG0,
	PK7, PG2,
	PK6, PK5,
	PK3, PK4,
	PK1, PK2

[static_digital_output yellow_led]
pins = !PB7

[board_pins]
aliases = 
	
	EXP1_1=PE6, EXP1_3=PG3, EXP1_5=PJ2, EXP1_7=PJ7, EXP1_9=<GND>,
	EXP1_2=PE2, EXP1_4=PG4, EXP1_6=PJ3, EXP1_8=PJ4, EXP1_10=<5V>,
	
	EXP2_1=PB3, EXP2_3=PJ5, EXP2_5=PJ6, EXP2_7=PD4, EXP2_9=<GND>,
	EXP2_2=PB1, EXP2_4=PB0, EXP2_6=PB2, EXP2_8=PE7, EXP2_10=PH2

[virtual_sdcard]
path = ~/taz/printer_data_taz/gcodes
on_error_gcode = CANCEL_PRINT

[pause_resume]

[display_status]

[respond]

[gcode_macro CANCEL_PRINT]
description = Cancel the actual running print
rename_existing = CANCEL_PRINT_BASE
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set allow_park = client.park_at_cancel|default(false)|lower == 'true' %}
	{% set retract = client.cancel_retract|default(5.0)|abs %}
	
	{% set park_x = "" if (client.park_at_cancel_x|default(none) is none)
	else "X=" ~ client.park_at_cancel_x %}
	{% set park_y = "" if (client.park_at_cancel_y|default(none) is none)
	else "Y=" ~ client.park_at_cancel_y %}
	{% set custom_park = park_x|length > 0 or park_y|length > 0 %}
	
	
	{% if printer['gcode_macro RESUME'].restore_idle_timeout > 0 %}
	SET_IDLE_TIMEOUT TIMEOUT={printer['gcode_macro RESUME'].restore_idle_timeout}
	{% endif %}
	{% if (custom_park or not printer.pause_resume.is_paused) and allow_park %} _TOOLHEAD_PARK_PAUSE_CANCEL {park_x} {park_y} {% endif %}
	_CLIENT_RETRACT LENGTH={retract}
	TURN_OFF_HEATERS
	M106 S0
	{client.user_cancel_macro|default("")}
	SET_GCODE_VARIABLE MACRO=RESUME VARIABLE=idle_state VALUE=False
	
	SET_PAUSE_NEXT_LAYER ENABLE=0
	SET_PAUSE_AT_LAYER ENABLE=0 LAYER=0
	CANCEL_PRINT_BASE

[gcode_macro PAUSE]
description = Pause the actual running print
rename_existing = PAUSE_BASE
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set idle_timeout = client.idle_timeout|default(0) %}
	{% set temp = printer[printer.toolhead.extruder].target if printer.toolhead.extruder != '' else 0 %}
	{% set restore = False if printer.toolhead.extruder == ''
	else True  if params.RESTORE|default(1)|int == 1 else False %}
	
	SET_GCODE_VARIABLE MACRO=RESUME VARIABLE=last_extruder_temp VALUE="{{'restore': restore, 'temp': temp}}"
	
	{% if idle_timeout > 0 %}
	SET_GCODE_VARIABLE MACRO=RESUME VARIABLE=restore_idle_timeout VALUE={printer.configfile.settings.idle_timeout.timeout}
	SET_IDLE_TIMEOUT TIMEOUT={idle_timeout}
	{% endif %}
	PAUSE_BASE
	{client.user_pause_macro|default("")}
	_TOOLHEAD_PARK_PAUSE_CANCEL {rawparams}

[gcode_macro RESUME]
description = Resume the actual running print
rename_existing = RESUME_BASE
variable_last_extruder_temp = {'restore': False, 'temp': 0}
variable_restore_idle_timeout = 0
variable_idle_state = False
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set velocity = printer.configfile.settings.pause_resume.recover_velocity %}
	{% set sp_move = client.speed_move|default(velocity) %}
	{% set runout_resume = True if client.runout_sensor|default("") == ""
	else True if not printer[client.runout_sensor].enabled
	else printer[client.runout_sensor].filament_detected %}
	{% set can_extrude = True if printer.toolhead.extruder == ''
	else printer[printer.toolhead.extruder].can_extrude %}
	{% set do_resume = False %}
	{% set prompt_txt = [] %}
	
	
	{% if printer.idle_timeout.state|upper == "IDLE" or idle_state %}
	SET_GCODE_VARIABLE MACRO=RESUME VARIABLE=idle_state VALUE=False
	{% if last_extruder_temp.restore %}
	
	RESPOND TYPE=echo MSG='{"Restoring \"%s\" temperature to %3.1f\u00B0C, this may take some time" % (printer.toolhead.extruder, last_extruder_temp.temp) }'
	M109 S{last_extruder_temp.temp}
	{% set do_resume = True %}
	{% elif can_extrude %}
	{% set do_resume = True %}
	{% else %}
	RESPOND TYPE=error MSG='{"Resume aborted !!! \"%s\" not hot enough, please heat up again and press RESUME" % printer.toolhead.extruder}'
	{% set _d = prompt_txt.append("\"%s\" not hot enough, please heat up again and press RESUME" % printer.toolhead.extruder) %}
	{% endif %}
	
	{% elif can_extrude %}
	{% set do_resume = True %}
	{% else %}
	RESPOND TYPE=error MSG='{"Resume aborted !!! \"%s\" not hot enough, please heat up again and press RESUME" % printer.toolhead.extruder}'
	{% set _d = prompt_txt.append("\"%s\" not hot enough, please heat up again and press RESUME" % printer.toolhead.extruder) %}
	{% endif %}
	{% if runout_resume %}
	{% if do_resume %}
	{% if restore_idle_timeout > 0 %} SET_IDLE_TIMEOUT TIMEOUT={restore_idle_timeout} {% endif %}
	{client.user_resume_macro|default("")}
	_CLIENT_EXTRUDE
	RESUME_BASE VELOCITY={params.VELOCITY|default(sp_move)}
	{% endif %}
	{% else %}
	RESPOND TYPE=error MSG='{"Resume aborted !!! \"%s\" detects no filament, please load filament and press RESUME" % (client.runout_sensor.split(" "))[1]}'
	{% set _d = prompt_txt.append("\"%s\" detects no filament, please load filament and press RESUME" % (client.runout_sensor.split(" "))[1]) %}
	{% endif %}
	
	{% if not (runout_resume and do_resume) %}
	RESPOND TYPE=command MSG="action:prompt_begin RESUME aborted !!!"
	{% for element in prompt_txt %}
	RESPOND TYPE=command MSG='{"action:prompt_text %s" % element}'
	{% endfor %}
	RESPOND TYPE=command MSG="action:prompt_footer_button Ok|RESPOND TYPE=command MSG=action:prompt_end|info"
	RESPOND TYPE=command MSG="action:prompt_show"
	{% endif %}

[gcode_macro SET_PAUSE_NEXT_LAYER]
description = Enable a pause if the next layer is reached
gcode = 
	{% set pause_next_layer = printer['gcode_macro SET_PRINT_STATS_INFO'].pause_next_layer %}
	{% set ENABLE = params.ENABLE|default(1)|int != 0 %}
	{% set MACRO = params.MACRO|default(pause_next_layer.call, True) %}
	SET_GCODE_VARIABLE MACRO=SET_PRINT_STATS_INFO VARIABLE=pause_next_layer VALUE="{{ 'enable': ENABLE, 'call': MACRO }}"

[gcode_macro SET_PAUSE_AT_LAYER]
description = Enable/disable a pause if a given layer number is reached
gcode = 
	{% set pause_at_layer = printer['gcode_macro SET_PRINT_STATS_INFO'].pause_at_layer %}
	{% set ENABLE = params.ENABLE|int != 0 if params.ENABLE is defined
	else params.LAYER is defined %}
	{% set LAYER = params.LAYER|default(pause_at_layer.layer)|int %}
	{% set MACRO = params.MACRO|default(pause_at_layer.call, True) %}
	SET_GCODE_VARIABLE MACRO=SET_PRINT_STATS_INFO VARIABLE=pause_at_layer VALUE="{{ 'enable': ENABLE, 'layer': LAYER, 'call': MACRO }}"

[gcode_macro SET_PRINT_STATS_INFO]
rename_existing = SET_PRINT_STATS_INFO_BASE
description = Overwrite, to get pause_next_layer and pause_at_layer feature
variable_pause_next_layer = { 'enable': False, 'call': "PAUSE" }
variable_pause_at_layer = { 'enable': False, 'layer': 0, 'call': "PAUSE" }
gcode = 
	{% if pause_next_layer.enable %}
	RESPOND TYPE=echo MSG='{"%s, forced by pause_next_layer" % pause_next_layer.call}'
	{pause_next_layer.call}
	SET_PAUSE_NEXT_LAYER ENABLE=0
	{% elif pause_at_layer.enable and params.CURRENT_LAYER is defined and params.CURRENT_LAYER|int == pause_at_layer.layer %}
	RESPOND TYPE=echo MSG='{"%s, forced by pause_at_layer [%d]" % (pause_at_layer.call, pause_at_layer.layer)}'
	{pause_at_layer.call}
	SET_PAUSE_AT_LAYER ENABLE=0
	{% endif %}
	SET_PRINT_STATS_INFO_BASE {rawparams}

[gcode_macro _TOOLHEAD_PARK_PAUSE_CANCEL]
description = Helper: park toolhead used in PAUSE and CANCEL_PRINT
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set velocity = printer.configfile.settings.pause_resume.recover_velocity %}
	{% set use_custom     = client.use_custom_pos|default(false)|lower == 'true' %}
	{% set custom_park_x  = client.custom_park_x|default(0.0) %}
	{% set custom_park_y  = client.custom_park_y|default(0.0) %}
	{% set park_dz        = client.custom_park_dz|default(2.0)|abs %}
	{% set sp_hop         = client.speed_hop|default(15) * 60 %}
	{% set sp_move        = client.speed_move|default(velocity) * 60 %}
	
	{% set origin    = printer.gcode_move.homing_origin %}
	{% set act       = printer.gcode_move.gcode_position %}
	{% set max       = printer.toolhead.axis_maximum %}
	{% set cone      = printer.toolhead.cone_start_z|default(max.z) %}
	{% set round_bed = True if printer.configfile.settings.printer.kinematics is in ['delta','polar','rotary_delta','winch']
	else False %}
	
	{% set z_min = params.Z_MIN|default(0)|float %}
	{% set z_park = [[(act.z + park_dz), z_min]|max, (max.z - origin.z)]|min %}
	{% set x_park = params.X       if params.X is defined
	else custom_park_x  if use_custom
	else 0.0            if round_bed
	else (max.x - 5.0) %}
	{% set y_park = params.Y       if params.Y is defined
	else custom_park_y  if use_custom
	else (max.y - 5.0)  if round_bed and z_park < cone
	else 0.0            if round_bed
	else (max.y - 5.0) %}
	
	_CLIENT_RETRACT
	{% if "xyz" in printer.toolhead.homed_axes %}
	G90
	G1 Z{z_park} F{sp_hop}
	G1 X{x_park} Y{y_park} F{sp_move}
	{% if not printer.gcode_move.absolute_coordinates %} G91 {% endif %}
	{% else %}
	RESPOND TYPE=echo MSG='Printer not homed'
	{% endif %}

[gcode_macro _CLIENT_EXTRUDE]
description = Extrudes, if the extruder is hot enough
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set use_fw_retract = (client.use_fw_retract|default(false)|lower == 'true') and (printer.firmware_retraction is defined) %}
	{% set length = params.LENGTH|default(client.unretract)|default(1.0)|float %}
	{% set speed = params.SPEED|default(client.speed_unretract)|default(35) %}
	{% set absolute_extrude = printer.gcode_move.absolute_extrude %}
	
	{% if printer.toolhead.extruder != '' %}
	{% if printer[printer.toolhead.extruder].can_extrude %}
	{% if use_fw_retract %}
	{% if length < 0 %}
	G10
	{% else %}
	G11
	{% endif %}
	{% else %}
	M83
	G1 E{length} F{(speed|float|abs) * 60}
	{% if absolute_extrude %}
	M82
	{% endif %}
	{% endif %}
	{% else %}
	RESPOND TYPE=echo MSG='{"\"%s\" not hot enough" % printer.toolhead.extruder}'
	{% endif %}
	{% endif %}

[gcode_macro _CLIENT_RETRACT]
description = Retracts, if the extruder is hot enough
gcode = 
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set length = params.LENGTH|default(client.retract)|default(1.0)|float %}
	{% set speed = params.SPEED|default(client.speed_retract)|default(35) %}
	
	_CLIENT_EXTRUDE LENGTH=-{length|float|abs} SPEED={speed|float|abs}

[bed_mesh default]
version = 1
points = 
	-1.065000, -0.857500, -0.817500, -0.865000, -0.927500
	-0.592500, -0.502500, -0.442500, -0.482500, -0.522500
	-0.172500, -0.070000, -0.027500, -0.040000, -0.057500
	0.182500, 0.265000, 0.312500, 0.302500, 0.332500
	0.480000, 0.610000, 0.670000, 0.715000, 0.735000
x_count = 5
y_count = 5
mesh_x_pps = 3
mesh_y_pps = 3
algo = bicubic
tension = 0.2
min_x = 30.0
max_x = 250.0
min_y = 39.989999999999995
max_y = 230.0
=======================
Loaded MCU 'mcu' 106 commands (v0.12.0-103-g6ce6fbbc / gcc: (GCC) 5.4.0 binutils: (GNU Binutils) 2.26.20160125)
MCU 'mcu' config: ADC_MAX=1023 BUS_PINS_spi=PB3,PB2,PB1 BUS_PINS_twi=PD0,PD1 CLOCK_FREQ=16000000 MCU=atmega2560 PWM_MAX=255 RECEIVE_WINDOW=192 RESERVE_PINS_serial=PE0,PE1 SERIAL_BAUD=250000 STATS_SUMSQ_BASE=256
Configured MCU 'mcu' (609 moves)
Args: ['/home/pi/taz/klipper-taz/klippy/klippy.py', '/home/pi/taz/printer_data_taz/config/printer.cfg', '-l', '/home/pi/taz/printer_data_taz/logs/klippy.log', '-I', '/home/pi/taz/printer_data_taz/comms/klippy.serial', '-a', '/home/pi/taz/printer_data_taz/comms/klippy.sock']
Git version: 'v0.12.0-103-g6ce6fbbc'
Branch: master
Remote: origin
Tracked URL: https://github.com/Klipper3d/klipper.git
CPU: 4 core ?
Python: '3.9.2 (default, Feb 28 2021, 17:03:44) \n[GCC 10.2.1 20210110]'
webhooks client 547750616272: {'program': 'Moonraker', 'version': 'v0.8.0-310-g67c98f6'}
=============== Log rollover at Fri Apr  5 19:56:07 2024 ===============
Attempting MCU 'mcu' reset
webhooks client 547750616272: Disconnected
Restarting printer
Start printer at Fri Apr  5 19:56:08 2024 (1712361368.8 1635650.5)
===== Config file =====
[gcode_macro CALIBRATE_NOZZLE_OFFSET]
description = Move to center of bed and calibrate nozzle offset
gcode = 
	G90
	G0 X100 Y155 F1500
	PROBE_CALIBRATE

[gcode_macro LEVEL_BED]
description = "Level the bed manually."
gcode = 
	BED_SCREWS_ADJUST

[gcode_macro CHECK_DEVIATION]
description = "Check the deviation of the bed from the last loaded mesh."
gcode = 
	SCREWS_TILT_CALCULATE MAX_DEVIATION=0.05

[gcode_macro LIZ_IS_A_BAKA]
description = "Liz is a baka, so here's her start G-Code >.<"
gcode = 
	BED_MESH_CALIBRATE
	BED_MESH_PROFILE SAVE=default

[gcode_macro _START_GCODE]
description = "The gcode that should be called from your slicer at the beginning of a print."
gcode = 
	
	G90
	G1 X2 Y30 Z30 F1500
	G1 Z0.28 F240
	G92 E0
	G1 Y220 E10 F1500
	G1 X2.3 F5000
	G92 E0
	G1 Y30 E10 F1200
	G92 E0
	G1 Z5 F1500

[gcode_macro _END_GCODE]
description = "The gcode that should be called from your slicer at the end of a print."
gcode = 
	G91
	G1 E-2 F2700
	G1 E-2 Z0.2 F2400
	G1 X5 Y5 F3000
	G1 Z10
	G90
	
	G1 X0 Y220
	M106 S0
	M104 S0
	M140 S0
	
	M84 X Y E

[stepper_x]
step_pin = PC0
dir_pin = PL1
enable_pin = !PA7
microsteps = 16
rotation_distance = 33
endstop_pin = ^!PB6
position_endstop = 0
position_max = 298
homing_speed = 50

[stepper_y]
step_pin = PC1
dir_pin = !PL0
enable_pin = !PA6
microsteps = 16
rotation_distance = 46
endstop_pin = ^!PB5
position_endstop = 0
position_max = 280
homing_speed = 50

[stepper_z]
step_pin = PC2
dir_pin = PL2
enable_pin = !PA5
microsteps = 16
rotation_distance = 8
endstop_pin = probe:z_virtual_endstop
position_max = 250

[bltouch]
sensor_pin = ^PB4
control_pin = PL5
x_offset = -44
y_offset = 8
z_offset = 2.850

[bed_mesh]
speed = 120
horizontal_move_z = 7
mesh_min = 30, 40
mesh_max = 250, 230
probe_count = 5
mesh_pps = 3
algorithm = bicubic

[safe_z_home]
home_xy_position = 140, 140
speed = 50
z_hop = 10
z_hop_speed = 5

[extruder]
step_pin = PC3
dir_pin = PL6
enable_pin = !PA4
microsteps = 16
rotation_distance = 7.9797
nozzle_diameter = 0.400
heater_pin = PH6
filament_diameter = 1.750
sensor_type = NTC 100K MGB18-104F39050L32
sensor_pin = PF0
min_temp = 0
max_temp = 990
control = pid
pid_kp = 23.769
pid_ki = 1.248
pid_kd = 113.201

[heater_bed]
heater_pin = PE5
sensor_type = EPCOS 100K B57560G104F
sensor_pin = PF2
control = watermark
min_temp = 0
max_temp = 130
max_power = 1.0

[verify_heater heater_bed]
heating_gain = 1
check_gain_time = 60

[fan]
pin = PH3

[heater_fan heatbreak_cooling_fan]
pin = PH5
fan_speed = 1.0
heater = extruder
heater_temp = 50.0

[mcu]
serial = /dev/serial/by-id/usb-UltiMachine__ultimachine.com__RAMBo_6403335373035101E171-if00
baud = 250000

[printer]
kinematics = cartesian
max_velocity = 300
max_accel = 3000
max_z_velocity = 5
max_z_accel = 100

[ad5206 stepper_digipot]
enable_pin = PD7
scale = 2.08
channel_1 = 1.34
channel_2 = 1.0
channel_4 = 1.1
channel_5 = 1.1
channel_6 = 1.1

[static_digital_output stepper_config]
pins = 
	PG1, PG0,
	PK7, PG2,
	PK6, PK5,
	PK3, PK4,
	PK1, PK2

[static_digital_output yellow_led]
pins = !PB7

[board_pins]
aliases = 
	
	EXP1_1=PE6, EXP1_3=PG3, EXP1_5=PJ2, EXP1_7=PJ7, EXP1_9=<GND>,
	EXP1_2=PE2, EXP1_4=PG4, EXP1_6=PJ3, EXP1_8=PJ4, EXP1_10=<5V>,
	
	EXP2_1=PB3, EXP2_3=PJ5, EXP2_5=PJ6, EXP2_7=PD4, EXP2_9=<GND>,
	EXP2_2=PB1, EXP2_4=PB0, EXP2_6=PB2, EXP2_8=PE7, EXP2_10=PH2

[virtual_sdcard]
path = ~/taz/printer_data_taz/gcodes
on_error_gcode = CANCEL_PRINT

[pause_resume]

[display_status]

[respond]

[gcode_macro CANCEL_PRINT]
description = Cancel the actual running print
rename_existing = CANCEL_PRINT_BASE
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set allow_park = client.park_at_cancel|default(false)|lower == 'true' %}
	{% set retract = client.cancel_retract|default(5.0)|abs %}
	
	{% set park_x = "" if (client.park_at_cancel_x|default(none) is none)
	else "X=" ~ client.park_at_cancel_x %}
	{% set park_y = "" if (client.park_at_cancel_y|default(none) is none)
	else "Y=" ~ client.park_at_cancel_y %}
	{% set custom_park = park_x|length > 0 or park_y|length > 0 %}
	
	
	{% if printer['gcode_macro RESUME'].restore_idle_timeout > 0 %}
	SET_IDLE_TIMEOUT TIMEOUT={printer['gcode_macro RESUME'].restore_idle_timeout}
	{% endif %}
	{% if (custom_park or not printer.pause_resume.is_paused) and allow_park %} _TOOLHEAD_PARK_PAUSE_CANCEL {park_x} {park_y} {% endif %}
	_CLIENT_RETRACT LENGTH={retract}
	TURN_OFF_HEATERS
	M106 S0
	{client.user_cancel_macro|default("")}
	SET_GCODE_VARIABLE MACRO=RESUME VARIABLE=idle_state VALUE=False
	
	SET_PAUSE_NEXT_LAYER ENABLE=0
	SET_PAUSE_AT_LAYER ENABLE=0 LAYER=0
	CANCEL_PRINT_BASE

[gcode_macro PAUSE]
description = Pause the actual running print
rename_existing = PAUSE_BASE
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set idle_timeout = client.idle_timeout|default(0) %}
	{% set temp = printer[printer.toolhead.extruder].target if printer.toolhead.extruder != '' else 0 %}
	{% set restore = False if printer.toolhead.extruder == ''
	else True  if params.RESTORE|default(1)|int == 1 else False %}
	
	SET_GCODE_VARIABLE MACRO=RESUME VARIABLE=last_extruder_temp VALUE="{{'restore': restore, 'temp': temp}}"
	
	{% if idle_timeout > 0 %}
	SET_GCODE_VARIABLE MACRO=RESUME VARIABLE=restore_idle_timeout VALUE={printer.configfile.settings.idle_timeout.timeout}
	SET_IDLE_TIMEOUT TIMEOUT={idle_timeout}
	{% endif %}
	PAUSE_BASE
	{client.user_pause_macro|default("")}
	_TOOLHEAD_PARK_PAUSE_CANCEL {rawparams}

[gcode_macro RESUME]
description = Resume the actual running print
rename_existing = RESUME_BASE
variable_last_extruder_temp = {'restore': False, 'temp': 0}
variable_restore_idle_timeout = 0
variable_idle_state = False
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set velocity = printer.configfile.settings.pause_resume.recover_velocity %}
	{% set sp_move = client.speed_move|default(velocity) %}
	{% set runout_resume = True if client.runout_sensor|default("") == ""
	else True if not printer[client.runout_sensor].enabled
	else printer[client.runout_sensor].filament_detected %}
	{% set can_extrude = True if printer.toolhead.extruder == ''
	else printer[printer.toolhead.extruder].can_extrude %}
	{% set do_resume = False %}
	{% set prompt_txt = [] %}
	
	
	{% if printer.idle_timeout.state|upper == "IDLE" or idle_state %}
	SET_GCODE_VARIABLE MACRO=RESUME VARIABLE=idle_state VALUE=False
	{% if last_extruder_temp.restore %}
	
	RESPOND TYPE=echo MSG='{"Restoring \"%s\" temperature to %3.1f\u00B0C, this may take some time" % (printer.toolhead.extruder, last_extruder_temp.temp) }'
	M109 S{last_extruder_temp.temp}
	{% set do_resume = True %}
	{% elif can_extrude %}
	{% set do_resume = True %}
	{% else %}
	RESPOND TYPE=error MSG='{"Resume aborted !!! \"%s\" not hot enough, please heat up again and press RESUME" % printer.toolhead.extruder}'
	{% set _d = prompt_txt.append("\"%s\" not hot enough, please heat up again and press RESUME" % printer.toolhead.extruder) %}
	{% endif %}
	
	{% elif can_extrude %}
	{% set do_resume = True %}
	{% else %}
	RESPOND TYPE=error MSG='{"Resume aborted !!! \"%s\" not hot enough, please heat up again and press RESUME" % printer.toolhead.extruder}'
	{% set _d = prompt_txt.append("\"%s\" not hot enough, please heat up again and press RESUME" % printer.toolhead.extruder) %}
	{% endif %}
	{% if runout_resume %}
	{% if do_resume %}
	{% if restore_idle_timeout > 0 %} SET_IDLE_TIMEOUT TIMEOUT={restore_idle_timeout} {% endif %}
	{client.user_resume_macro|default("")}
	_CLIENT_EXTRUDE
	RESUME_BASE VELOCITY={params.VELOCITY|default(sp_move)}
	{% endif %}
	{% else %}
	RESPOND TYPE=error MSG='{"Resume aborted !!! \"%s\" detects no filament, please load filament and press RESUME" % (client.runout_sensor.split(" "))[1]}'
	{% set _d = prompt_txt.append("\"%s\" detects no filament, please load filament and press RESUME" % (client.runout_sensor.split(" "))[1]) %}
	{% endif %}
	
	{% if not (runout_resume and do_resume) %}
	RESPOND TYPE=command MSG="action:prompt_begin RESUME aborted !!!"
	{% for element in prompt_txt %}
	RESPOND TYPE=command MSG='{"action:prompt_text %s" % element}'
	{% endfor %}
	RESPOND TYPE=command MSG="action:prompt_footer_button Ok|RESPOND TYPE=command MSG=action:prompt_end|info"
	RESPOND TYPE=command MSG="action:prompt_show"
	{% endif %}

[gcode_macro SET_PAUSE_NEXT_LAYER]
description = Enable a pause if the next layer is reached
gcode = 
	{% set pause_next_layer = printer['gcode_macro SET_PRINT_STATS_INFO'].pause_next_layer %}
	{% set ENABLE = params.ENABLE|default(1)|int != 0 %}
	{% set MACRO = params.MACRO|default(pause_next_layer.call, True) %}
	SET_GCODE_VARIABLE MACRO=SET_PRINT_STATS_INFO VARIABLE=pause_next_layer VALUE="{{ 'enable': ENABLE, 'call': MACRO }}"

[gcode_macro SET_PAUSE_AT_LAYER]
description = Enable/disable a pause if a given layer number is reached
gcode = 
	{% set pause_at_layer = printer['gcode_macro SET_PRINT_STATS_INFO'].pause_at_layer %}
	{% set ENABLE = params.ENABLE|int != 0 if params.ENABLE is defined
	else params.LAYER is defined %}
	{% set LAYER = params.LAYER|default(pause_at_layer.layer)|int %}
	{% set MACRO = params.MACRO|default(pause_at_layer.call, True) %}
	SET_GCODE_VARIABLE MACRO=SET_PRINT_STATS_INFO VARIABLE=pause_at_layer VALUE="{{ 'enable': ENABLE, 'layer': LAYER, 'call': MACRO }}"

[gcode_macro SET_PRINT_STATS_INFO]
rename_existing = SET_PRINT_STATS_INFO_BASE
description = Overwrite, to get pause_next_layer and pause_at_layer feature
variable_pause_next_layer = { 'enable': False, 'call': "PAUSE" }
variable_pause_at_layer = { 'enable': False, 'layer': 0, 'call': "PAUSE" }
gcode = 
	{% if pause_next_layer.enable %}
	RESPOND TYPE=echo MSG='{"%s, forced by pause_next_layer" % pause_next_layer.call}'
	{pause_next_layer.call}
	SET_PAUSE_NEXT_LAYER ENABLE=0
	{% elif pause_at_layer.enable and params.CURRENT_LAYER is defined and params.CURRENT_LAYER|int == pause_at_layer.layer %}
	RESPOND TYPE=echo MSG='{"%s, forced by pause_at_layer [%d]" % (pause_at_layer.call, pause_at_layer.layer)}'
	{pause_at_layer.call}
	SET_PAUSE_AT_LAYER ENABLE=0
	{% endif %}
	SET_PRINT_STATS_INFO_BASE {rawparams}

[gcode_macro _TOOLHEAD_PARK_PAUSE_CANCEL]
description = Helper: park toolhead used in PAUSE and CANCEL_PRINT
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set velocity = printer.configfile.settings.pause_resume.recover_velocity %}
	{% set use_custom     = client.use_custom_pos|default(false)|lower == 'true' %}
	{% set custom_park_x  = client.custom_park_x|default(0.0) %}
	{% set custom_park_y  = client.custom_park_y|default(0.0) %}
	{% set park_dz        = client.custom_park_dz|default(2.0)|abs %}
	{% set sp_hop         = client.speed_hop|default(15) * 60 %}
	{% set sp_move        = client.speed_move|default(velocity) * 60 %}
	
	{% set origin    = printer.gcode_move.homing_origin %}
	{% set act       = printer.gcode_move.gcode_position %}
	{% set max       = printer.toolhead.axis_maximum %}
	{% set cone      = printer.toolhead.cone_start_z|default(max.z) %}
	{% set round_bed = True if printer.configfile.settings.printer.kinematics is in ['delta','polar','rotary_delta','winch']
	else False %}
	
	{% set z_min = params.Z_MIN|default(0)|float %}
	{% set z_park = [[(act.z + park_dz), z_min]|max, (max.z - origin.z)]|min %}
	{% set x_park = params.X       if params.X is defined
	else custom_park_x  if use_custom
	else 0.0            if round_bed
	else (max.x - 5.0) %}
	{% set y_park = params.Y       if params.Y is defined
	else custom_park_y  if use_custom
	else (max.y - 5.0)  if round_bed and z_park < cone
	else 0.0            if round_bed
	else (max.y - 5.0) %}
	
	_CLIENT_RETRACT
	{% if "xyz" in printer.toolhead.homed_axes %}
	G90
	G1 Z{z_park} F{sp_hop}
	G1 X{x_park} Y{y_park} F{sp_move}
	{% if not printer.gcode_move.absolute_coordinates %} G91 {% endif %}
	{% else %}
	RESPOND TYPE=echo MSG='Printer not homed'
	{% endif %}

[gcode_macro _CLIENT_EXTRUDE]
description = Extrudes, if the extruder is hot enough
gcode = 
	
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set use_fw_retract = (client.use_fw_retract|default(false)|lower == 'true') and (printer.firmware_retraction is defined) %}
	{% set length = params.LENGTH|default(client.unretract)|default(1.0)|float %}
	{% set speed = params.SPEED|default(client.speed_unretract)|default(35) %}
	{% set absolute_extrude = printer.gcode_move.absolute_extrude %}
	
	{% if printer.toolhead.extruder != '' %}
	{% if printer[printer.toolhead.extruder].can_extrude %}
	{% if use_fw_retract %}
	{% if length < 0 %}
	G10
	{% else %}
	G11
	{% endif %}
	{% else %}
	M83
	G1 E{length} F{(speed|float|abs) * 60}
	{% if absolute_extrude %}
	M82
	{% endif %}
	{% endif %}
	{% else %}
	RESPOND TYPE=echo MSG='{"\"%s\" not hot enough" % printer.toolhead.extruder}'
	{% endif %}
	{% endif %}

[gcode_macro _CLIENT_RETRACT]
description = Retracts, if the extruder is hot enough
gcode = 
	{% set client = printer['gcode_macro _CLIENT_VARIABLE']|default({}) %}
	{% set length = params.LENGTH|default(client.retract)|default(1.0)|float %}
	{% set speed = params.SPEED|default(client.speed_retract)|default(35) %}
	
	_CLIENT_EXTRUDE LENGTH=-{length|float|abs} SPEED={speed|float|abs}

[bed_mesh default]
version = 1
points = 
	-1.065000, -0.857500, -0.817500, -0.865000, -0.927500
	-0.592500, -0.502500, -0.442500, -0.482500, -0.522500
	-0.172500, -0.070000, -0.027500, -0.040000, -0.057500
	0.182500, 0.265000, 0.312500, 0.302500, 0.332500
	0.480000, 0.610000, 0.670000, 0.715000, 0.735000
x_count = 5
y_count = 5
mesh_x_pps = 3
mesh_y_pps = 3
algo = bicubic
tension = 0.2
min_x = 30.0
max_x = 250.0
min_y = 39.989999999999995
max_y = 230.0
=======================
Extruder max_extrude_ratio=0.266081
mcu 'mcu': Starting serial connect
webhooks client 547757213248: New connection
webhooks client 547757213248: Client info {'program': 'Moonraker', 'version': 'v0.8.0-310-g67c98f6'}
Loaded MCU 'mcu' 106 commands (v0.12.0-103-g6ce6fbbc / gcc: (GCC) 5.4.0 binutils: (GNU Binutils) 2.26.20160125)
MCU 'mcu' config: ADC_MAX=1023 BUS_PINS_spi=PB3,PB2,PB1 BUS_PINS_twi=PD0,PD1 CLOCK_FREQ=16000000 MCU=atmega2560 PWM_MAX=255 RECEIVE_WINDOW=192 RESERVE_PINS_serial=PE0,PE1 SERIAL_BAUD=250000 STATS_SUMSQ_BASE=256
Sending MCU 'mcu' printer configuration...
Configured MCU 'mcu' (609 moves)
bed_mesh: generated points
Index |  Tool Adjusted  |   Probe
  0   | (74.0, 32.0)    | (30.0, 40.0)
  1   | (129.0, 32.0)   | (85.0, 40.0)
  2   | (184.0, 32.0)   | (140.0, 40.0)
  3   | (239.0, 32.0)   | (195.0, 40.0)
  4   | (294.0, 32.0)   | (250.0, 40.0)
  5   | (294.0, 79.5)   | (250.0, 87.5)
  6   | (239.0, 79.5)   | (195.0, 87.5)
  7   | (184.0, 79.5)   | (140.0, 87.5)
  8   | (129.0, 79.5)   | (85.0, 87.5)
  9   | (74.0, 79.5)    | (30.0, 87.5)
  10  | (74.0, 127.0)   | (30.0, 135.0)
  11  | (129.0, 127.0)  | (85.0, 135.0)
  12  | (184.0, 127.0)  | (140.0, 135.0)
  13  | (239.0, 127.0)  | (195.0, 135.0)
  14  | (294.0, 127.0)  | (250.0, 135.0)
  15  | (294.0, 174.5)  | (250.0, 182.5)
  16  | (239.0, 174.5)  | (195.0, 182.5)
  17  | (184.0, 174.5)  | (140.0, 182.5)
  18  | (129.0, 174.5)  | (85.0, 182.5)
  19  | (74.0, 174.5)   | (30.0, 182.5)
  20  | (74.0, 222.0)   | (30.0, 230.0)
  21  | (129.0, 222.0)  | (85.0, 230.0)
  22  | (184.0, 222.0)  | (140.0, 230.0)
  23  | (239.0, 222.0)  | (195.0, 230.0)
  24  | (294.0, 222.0)  | (250.0, 230.0)
Starting heater checks for heater_bed
Starting heater checks for extruder
Write g-code response
Traceback (most recent call last):
  File "/home/pi/taz/klipper-taz/klippy/gcode.py", line 459, in _respond_raw
    os.write(self.fd, (msg+"\n").encode())
BlockingIOError: [Errno 11] Resource temporarily unavailable
Stats 1635652.7: gcodein=0  mcu: mcu_awake=0.000 mcu_task_avg=0.000000 mcu_task_stddev=0.000000 bytes_write=1209 bytes_read=4112 bytes_retransmit=0 bytes_invalid=0 send_seq=126 receive_seq=125 retransmit_seq=0 srtt=0.003 rttvar=0.000 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999674 heater_bed: target=0 temp=0.0 pwm=0.000  sysload=0.10 cputime=14247.348 memavail=7381728 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=0.0 pwm=0.000
webhooks: registering remote method 'shutdown_machine' for connection id: 547757213248
webhooks: registering remote method 'reboot_machine' for connection id: 547757213248
webhooks: registering remote method 'pause_job_queue' for connection id: 547757213248
webhooks: registering remote method 'start_job_queue' for connection id: 547757213248
Stats 1635653.7: gcodein=0  mcu: mcu_awake=0.000 mcu_task_avg=0.000000 mcu_task_stddev=0.000000 bytes_write=1215 bytes_read=4197 bytes_retransmit=0 bytes_invalid=0 send_seq=127 receive_seq=127 retransmit_seq=0 srtt=0.003 rttvar=0.000 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999388 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.10 cputime=14247.364 memavail=7381256 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635654.7: gcodein=0  mcu: mcu_awake=0.000 mcu_task_avg=0.000000 mcu_task_stddev=0.000000 bytes_write=1221 bytes_read=4303 bytes_retransmit=0 bytes_invalid=0 send_seq=128 receive_seq=128 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999256 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.09 cputime=14247.378 memavail=7384716 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635655.7: gcodein=0  mcu: mcu_awake=0.000 mcu_task_avg=0.000000 mcu_task_stddev=0.000000 bytes_write=1227 bytes_read=4396 bytes_retransmit=0 bytes_invalid=0 send_seq=129 receive_seq=129 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999278 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.09 cputime=14247.388 memavail=7384832 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635656.7: gcodein=0  mcu: mcu_awake=0.031 mcu_task_avg=0.000153 mcu_task_stddev=0.000365 bytes_write=1233 bytes_read=4517 bytes_retransmit=0 bytes_invalid=0 send_seq=130 receive_seq=130 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999280 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.09 cputime=14247.401 memavail=7384580 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635657.7: gcodein=0  mcu: mcu_awake=0.031 mcu_task_avg=0.000153 mcu_task_stddev=0.000365 bytes_write=1239 bytes_read=4623 bytes_retransmit=0 bytes_invalid=0 send_seq=131 receive_seq=131 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999284 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.09 cputime=14247.413 memavail=7383856 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635658.7: gcodein=0  mcu: mcu_awake=0.031 mcu_task_avg=0.000153 mcu_task_stddev=0.000365 bytes_write=1245 bytes_read=4716 bytes_retransmit=0 bytes_invalid=0 send_seq=132 receive_seq=132 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999278 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.09 cputime=14247.425 memavail=7383856 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635659.7: gcodein=0  mcu: mcu_awake=0.031 mcu_task_avg=0.000153 mcu_task_stddev=0.000365 bytes_write=1251 bytes_read=4822 bytes_retransmit=0 bytes_invalid=0 send_seq=133 receive_seq=133 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999267 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.09 cputime=14247.438 memavail=7383856 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635660.7: gcodein=0  mcu: mcu_awake=0.031 mcu_task_avg=0.000153 mcu_task_stddev=0.000365 bytes_write=1257 bytes_read=4928 bytes_retransmit=0 bytes_invalid=0 send_seq=134 receive_seq=134 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999268 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.09 cputime=14247.450 memavail=7375520 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635661.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000074 mcu_task_stddev=0.000059 bytes_write=1263 bytes_read=5034 bytes_retransmit=0 bytes_invalid=0 send_seq=135 receive_seq=135 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999247 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.09 cputime=14247.459 memavail=7381916 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635662.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000074 mcu_task_stddev=0.000059 bytes_write=1269 bytes_read=5140 bytes_retransmit=0 bytes_invalid=0 send_seq=136 receive_seq=136 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999236 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.09 cputime=14247.467 memavail=7381916 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.0 pwm=0.000
Stats 1635663.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000074 mcu_task_stddev=0.000059 bytes_write=1275 bytes_read=5250 bytes_retransmit=0 bytes_invalid=0 send_seq=137 receive_seq=137 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999233 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.09 cputime=14247.474 memavail=7381916 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635664.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000074 mcu_task_stddev=0.000059 bytes_write=1281 bytes_read=5350 bytes_retransmit=0 bytes_invalid=0 send_seq=138 receive_seq=138 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999223 heater_bed: target=0 temp=20.9 pwm=0.000  sysload=0.08 cputime=14247.482 memavail=7381336 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635665.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000074 mcu_task_stddev=0.000059 bytes_write=1287 bytes_read=5464 bytes_retransmit=0 bytes_invalid=0 send_seq=139 receive_seq=139 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999232 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.08 cputime=14247.492 memavail=7381336 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635666.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000063 bytes_write=1293 bytes_read=5591 bytes_retransmit=0 bytes_invalid=0 send_seq=140 receive_seq=140 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999233 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.08 cputime=14247.506 memavail=7381440 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635667.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000063 bytes_write=1299 bytes_read=5691 bytes_retransmit=0 bytes_invalid=0 send_seq=141 receive_seq=141 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999241 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.08 cputime=14247.519 memavail=7382196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635668.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000063 bytes_write=1305 bytes_read=5805 bytes_retransmit=0 bytes_invalid=0 send_seq=142 receive_seq=142 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999238 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.08 cputime=14247.532 memavail=7382196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635669.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000063 bytes_write=1311 bytes_read=5919 bytes_retransmit=0 bytes_invalid=0 send_seq=143 receive_seq=143 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999238 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.546 memavail=7382196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635670.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000063 bytes_write=1317 bytes_read=6019 bytes_retransmit=0 bytes_invalid=0 send_seq=144 receive_seq=144 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999239 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.558 memavail=7382196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635671.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=1323 bytes_read=6146 bytes_retransmit=0 bytes_invalid=0 send_seq=145 receive_seq=145 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999236 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.572 memavail=7382196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635672.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=1329 bytes_read=6260 bytes_retransmit=0 bytes_invalid=0 send_seq=146 receive_seq=146 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999233 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.585 memavail=7382196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635673.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=1335 bytes_read=6360 bytes_retransmit=0 bytes_invalid=0 send_seq=147 receive_seq=147 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999233 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.598 memavail=7382196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635674.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=1341 bytes_read=6474 bytes_retransmit=0 bytes_invalid=0 send_seq=148 receive_seq=148 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999232 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.611 memavail=7381700 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635675.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=1347 bytes_read=6588 bytes_retransmit=0 bytes_invalid=0 send_seq=149 receive_seq=149 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999231 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.624 memavail=7381700 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635676.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1353 bytes_read=6701 bytes_retransmit=0 bytes_invalid=0 send_seq=150 receive_seq=150 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999230 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.637 memavail=7381700 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635677.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1359 bytes_read=6815 bytes_retransmit=0 bytes_invalid=0 send_seq=151 receive_seq=151 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999230 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.650 memavail=7381196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635678.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1365 bytes_read=6929 bytes_retransmit=0 bytes_invalid=0 send_seq=152 receive_seq=152 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999230 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.07 cputime=14247.663 memavail=7381196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635679.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1371 bytes_read=7029 bytes_retransmit=0 bytes_invalid=0 send_seq=153 receive_seq=153 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999227 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.06 cputime=14247.677 memavail=7381196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635680.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1377 bytes_read=7143 bytes_retransmit=0 bytes_invalid=0 send_seq=154 receive_seq=154 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999226 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.06 cputime=14247.691 memavail=7381196 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635681.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000082 mcu_task_stddev=0.000068 bytes_write=1383 bytes_read=7270 bytes_retransmit=0 bytes_invalid=0 send_seq=155 receive_seq=155 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999225 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.06 cputime=14247.707 memavail=7380944 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635682.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000082 mcu_task_stddev=0.000068 bytes_write=1389 bytes_read=7370 bytes_retransmit=0 bytes_invalid=0 send_seq=156 receive_seq=156 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999223 heater_bed: target=0 temp=20.3 pwm=0.000  sysload=0.06 cputime=14247.715 memavail=7380444 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.5 pwm=0.000
Stats 1635683.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000082 mcu_task_stddev=0.000068 bytes_write=1395 bytes_read=7484 bytes_retransmit=0 bytes_invalid=0 send_seq=157 receive_seq=157 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999223 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.06 cputime=14247.724 memavail=7372148 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635684.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000082 mcu_task_stddev=0.000068 bytes_write=1401 bytes_read=7598 bytes_retransmit=0 bytes_invalid=0 send_seq=158 receive_seq=158 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999220 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.22 cputime=14247.734 memavail=7367268 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635685.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000082 mcu_task_stddev=0.000068 bytes_write=1407 bytes_read=7698 bytes_retransmit=0 bytes_invalid=0 send_seq=159 receive_seq=159 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999219 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.22 cputime=14247.744 memavail=7367008 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635686.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1413 bytes_read=7825 bytes_retransmit=0 bytes_invalid=0 send_seq=160 receive_seq=160 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999230 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.22 cputime=14247.754 memavail=7367044 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=20.9 pwm=0.000
Stats 1635687.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1419 bytes_read=7939 bytes_retransmit=0 bytes_invalid=0 send_seq=161 receive_seq=161 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999226 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.22 cputime=14247.765 memavail=7366004 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635688.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1425 bytes_read=8039 bytes_retransmit=0 bytes_invalid=0 send_seq=162 receive_seq=162 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999223 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.22 cputime=14247.775 memavail=7366480 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=20.8 pwm=0.000
Stats 1635689.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1431 bytes_read=8167 bytes_retransmit=0 bytes_invalid=0 send_seq=163 receive_seq=163 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999222 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.28 cputime=14247.784 memavail=7366752 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635690.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1437 bytes_read=8267 bytes_retransmit=0 bytes_invalid=0 send_seq=164 receive_seq=164 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999220 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.28 cputime=14247.794 memavail=7366424 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635691.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=1443 bytes_read=8380 bytes_retransmit=0 bytes_invalid=0 send_seq=165 receive_seq=165 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999218 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.28 cputime=14247.803 memavail=7366772 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635692.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=1449 bytes_read=8508 bytes_retransmit=0 bytes_invalid=0 send_seq=166 receive_seq=166 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999219 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.28 cputime=14247.816 memavail=7369056 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635693.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=1455 bytes_read=8608 bytes_retransmit=0 bytes_invalid=0 send_seq=167 receive_seq=167 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999217 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.28 cputime=14247.826 memavail=7367692 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635694.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=1461 bytes_read=8708 bytes_retransmit=0 bytes_invalid=0 send_seq=168 receive_seq=168 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999216 heater_bed: target=0 temp=20.8 pwm=0.000  sysload=0.34 cputime=14247.835 memavail=7370440 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635695.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=1467 bytes_read=8836 bytes_retransmit=0 bytes_invalid=0 send_seq=169 receive_seq=169 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999214 heater_bed: target=0 temp=20.8 pwm=0.000  sysload=0.34 cputime=14247.846 memavail=7366744 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635696.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1473 bytes_read=8949 bytes_retransmit=0 bytes_invalid=0 send_seq=170 receive_seq=170 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.34 cputime=14247.857 memavail=7335860 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635697.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1479 bytes_read=9049 bytes_retransmit=0 bytes_invalid=0 send_seq=171 receive_seq=171 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.34 cputime=14247.867 memavail=7309556 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635698.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1485 bytes_read=9177 bytes_retransmit=0 bytes_invalid=0 send_seq=172 receive_seq=172 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.34 cputime=14247.880 memavail=7266236 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635699.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1491 bytes_read=9277 bytes_retransmit=0 bytes_invalid=0 send_seq=173 receive_seq=173 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.55 cputime=14247.890 memavail=7232756 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635700.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=1497 bytes_read=9377 bytes_retransmit=0 bytes_invalid=0 send_seq=174 receive_seq=174 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.55 cputime=14247.899 memavail=7225676 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=20.9 pwm=0.000
Stats 1635701.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1503 bytes_read=9518 bytes_retransmit=0 bytes_invalid=0 send_seq=175 receive_seq=175 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.55 cputime=14247.907 memavail=7225676 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635702.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1509 bytes_read=9618 bytes_retransmit=0 bytes_invalid=0 send_seq=176 receive_seq=176 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.55 cputime=14247.917 memavail=7218116 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635703.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1515 bytes_read=9718 bytes_retransmit=0 bytes_invalid=0 send_seq=177 receive_seq=177 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.55 cputime=14247.927 memavail=7191116 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635704.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1521 bytes_read=9846 bytes_retransmit=0 bytes_invalid=0 send_seq=178 receive_seq=178 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.67 cputime=14247.937 memavail=7186652 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635705.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1527 bytes_read=9946 bytes_retransmit=0 bytes_invalid=0 send_seq=179 receive_seq=179 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.67 cputime=14247.946 memavail=7185448 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635706.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1533 bytes_read=10059 bytes_retransmit=0 bytes_invalid=0 send_seq=180 receive_seq=180 retransmit_seq=0 srtt=0.002 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.67 cputime=14247.955 memavail=7183640 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635707.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1539 bytes_read=10187 bytes_retransmit=0 bytes_invalid=0 send_seq=181 receive_seq=181 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.67 cputime=14247.964 memavail=7185408 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635708.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1545 bytes_read=10287 bytes_retransmit=0 bytes_invalid=0 send_seq=182 receive_seq=182 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999214 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.67 cputime=14247.977 memavail=7185320 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635709.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1551 bytes_read=10387 bytes_retransmit=0 bytes_invalid=0 send_seq=183 receive_seq=183 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999218 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.69 cputime=14247.991 memavail=7187040 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635710.7: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=1563 bytes_read=10531 bytes_retransmit=0 bytes_invalid=0 send_seq=185 receive_seq=185 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999216 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.69 cputime=14248.004 memavail=7187044 print_time=0.000 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635771.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=2141 bytes_read=17367 bytes_retransmit=0 bytes_invalid=0 send_seq=250 receive_seq=250 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.44 cputime=14248.699 memavail=7220568 print_time=122.418 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635772.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000093 mcu_task_stddev=0.000100 bytes_write=2153 bytes_read=17512 bytes_retransmit=0 bytes_invalid=0 send_seq=252 receive_seq=252 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.44 cputime=14248.714 memavail=7220568 print_time=122.418 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635773.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000093 mcu_task_stddev=0.000100 bytes_write=2505 bytes_read=17762 bytes_retransmit=0 bytes_invalid=0 send_seq=269 receive_seq=269 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.44 cputime=14248.741 memavail=7220568 print_time=123.042 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635774.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000093 mcu_task_stddev=0.000100 bytes_write=2899 bytes_read=18156 bytes_retransmit=0 bytes_invalid=0 send_seq=298 receive_seq=298 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.41 cputime=14248.783 memavail=7221752 print_time=124.006 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635775.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000093 mcu_task_stddev=0.000100 bytes_write=3431 bytes_read=18661 bytes_retransmit=0 bytes_invalid=0 send_seq=335 receive_seq=335 retransmit_seq=0 srtt=0.003 rttvar=0.000 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.41 cputime=14248.825 memavail=7221828 print_time=125.186 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635776.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000093 mcu_task_stddev=0.000100 bytes_write=4076 bytes_read=18994 bytes_retransmit=0 bytes_invalid=0 send_seq=360 receive_seq=360 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=26 freq=15999213 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.41 cputime=14248.862 memavail=7221828 print_time=129.777 buffer_time=3.924 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635777.8: gcodein=0  mcu: mcu_awake=0.032 mcu_task_avg=0.000131 mcu_task_stddev=0.000109 bytes_write=4082 bytes_read=19109 bytes_retransmit=0 bytes_invalid=0 send_seq=361 receive_seq=361 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=26 freq=15999213 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.41 cputime=14248.872 memavail=7238464 print_time=129.777 buffer_time=2.924 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635778.8: gcodein=0  mcu: mcu_awake=0.032 mcu_task_avg=0.000131 mcu_task_stddev=0.000109 bytes_write=4088 bytes_read=19223 bytes_retransmit=0 bytes_invalid=0 send_seq=362 receive_seq=362 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=26 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.41 cputime=14248.881 memavail=7238464 print_time=129.777 buffer_time=1.924 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635779.8: gcodein=0  mcu: mcu_awake=0.032 mcu_task_avg=0.000131 mcu_task_stddev=0.000109 bytes_write=4094 bytes_read=19337 bytes_retransmit=0 bytes_invalid=0 send_seq=363 receive_seq=363 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=26 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.37 cputime=14248.889 memavail=7238464 print_time=129.777 buffer_time=0.923 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635780.8: gcodein=0  mcu: mcu_awake=0.032 mcu_task_avg=0.000131 mcu_task_stddev=0.000109 bytes_write=4100 bytes_read=19437 bytes_retransmit=0 bytes_invalid=0 send_seq=364 receive_seq=364 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=8 upcoming_bytes=18 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.37 cputime=14248.897 memavail=7238112 print_time=129.777 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635781.8: gcodein=0  mcu: mcu_awake=0.032 mcu_task_avg=0.000131 mcu_task_stddev=0.000109 bytes_write=4244 bytes_read=19667 bytes_retransmit=0 bytes_invalid=0 send_seq=374 receive_seq=374 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=8 upcoming_bytes=0 freq=15999214 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.37 cputime=14248.912 memavail=7243348 print_time=131.507 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635782.8: gcodein=0  mcu: mcu_awake=0.011 mcu_task_avg=0.000101 mcu_task_stddev=0.000084 bytes_write=4479 bytes_read=19936 bytes_retransmit=0 bytes_invalid=0 send_seq=389 receive_seq=389 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999214 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.37 cputime=14248.934 memavail=7243348 print_time=132.007 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635783.8: gcodein=0  mcu: mcu_awake=0.011 mcu_task_avg=0.000101 mcu_task_stddev=0.000084 bytes_write=4893 bytes_read=20383 bytes_retransmit=0 bytes_invalid=0 send_seq=424 receive_seq=423 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.37 cputime=14248.969 memavail=7243348 print_time=133.057 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635784.8: gcodein=0  mcu: mcu_awake=0.011 mcu_task_avg=0.000101 mcu_task_stddev=0.000084 bytes_write=5295 bytes_read=20863 bytes_retransmit=0 bytes_invalid=0 send_seq=458 receive_seq=458 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.34 cputime=14249.004 memavail=7243124 print_time=134.007 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635785.8: gcodein=0  mcu: mcu_awake=0.011 mcu_task_avg=0.000101 mcu_task_stddev=0.000084 bytes_write=5692 bytes_read=21319 bytes_retransmit=0 bytes_invalid=0 send_seq=491 receive_seq=491 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.34 cputime=14249.038 memavail=7243124 print_time=135.007 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635786.8: gcodein=0  mcu: mcu_awake=0.011 mcu_task_avg=0.000101 mcu_task_stddev=0.000084 bytes_write=6101 bytes_read=21761 bytes_retransmit=0 bytes_invalid=0 send_seq=525 receive_seq=524 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.34 cputime=14249.074 memavail=7243124 print_time=136.057 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635787.8: gcodein=0  mcu: mcu_awake=0.039 mcu_task_avg=0.000120 mcu_task_stddev=0.000050 bytes_write=6515 bytes_read=22256 bytes_retransmit=0 bytes_invalid=0 send_seq=560 receive_seq=559 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.34 cputime=14249.109 memavail=7242368 print_time=137.057 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635788.8: gcodein=0  mcu: mcu_awake=0.039 mcu_task_avg=0.000120 mcu_task_stddev=0.000050 bytes_write=6911 bytes_read=22619 bytes_retransmit=0 bytes_invalid=0 send_seq=581 receive_seq=581 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=16 upcoming_bytes=8 freq=15999212 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.34 cputime=14249.145 memavail=7242372 print_time=139.753 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635789.8: gcodein=0  mcu: mcu_awake=0.039 mcu_task_avg=0.000120 mcu_task_stddev=0.000050 bytes_write=6933 bytes_read=22719 bytes_retransmit=0 bytes_invalid=0 send_seq=582 receive_seq=582 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=8 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.32 cputime=14249.159 memavail=7242372 print_time=139.753 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635790.8: gcodein=0  mcu: mcu_awake=0.039 mcu_task_avg=0.000120 mcu_task_stddev=0.000050 bytes_write=7073 bytes_read=22901 bytes_retransmit=0 bytes_invalid=0 send_seq=591 receive_seq=591 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.3 pwm=0.000  sysload=0.32 cputime=14249.180 memavail=7242372 print_time=140.053 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635791.8: gcodein=0  mcu: mcu_awake=0.039 mcu_task_avg=0.000120 mcu_task_stddev=0.000050 bytes_write=7475 bytes_read=23362 bytes_retransmit=0 bytes_invalid=0 send_seq=625 receive_seq=625 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.3 pwm=0.000  sysload=0.32 cputime=14249.217 memavail=7242372 print_time=141.053 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635792.8: gcodein=0  mcu: mcu_awake=0.026 mcu_task_avg=0.000115 mcu_task_stddev=0.000075 bytes_write=7884 bytes_read=23864 bytes_retransmit=0 bytes_invalid=0 send_seq=661 receive_seq=661 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=45 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.32 cputime=14249.253 memavail=7242372 print_time=141.945 buffer_time=0.086 print_stall=0 extruder: target=0 temp=20.9 pwm=0.000
Stats 1635793.8: gcodein=0  mcu: mcu_awake=0.026 mcu_task_avg=0.000115 mcu_task_stddev=0.000075 bytes_write=8090 bytes_read=24095 bytes_retransmit=0 bytes_invalid=0 send_seq=671 receive_seq=671 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.32 cputime=14249.276 memavail=7242372 print_time=144.326 buffer_time=1.465 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635794.8: gcodein=0  mcu: mcu_awake=0.026 mcu_task_avg=0.000115 mcu_task_stddev=0.000075 bytes_write=8096 bytes_read=24209 bytes_retransmit=0 bytes_invalid=0 send_seq=672 receive_seq=672 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.29 cputime=14249.290 memavail=7242372 print_time=144.326 buffer_time=0.465 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635795.8: gcodein=0  mcu: mcu_awake=0.026 mcu_task_avg=0.000115 mcu_task_stddev=0.000075 bytes_write=8160 bytes_read=24314 bytes_retransmit=0 bytes_invalid=0 send_seq=674 receive_seq=674 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.29 cputime=14249.306 memavail=7242372 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635796.8: gcodein=0  mcu: mcu_awake=0.026 mcu_task_avg=0.000115 mcu_task_stddev=0.000075 bytes_write=8166 bytes_read=24428 bytes_retransmit=0 bytes_invalid=0 send_seq=675 receive_seq=675 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.29 cputime=14249.321 memavail=7242372 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635797.8: gcodein=0  mcu: mcu_awake=0.012 mcu_task_avg=0.000098 mcu_task_stddev=0.000086 bytes_write=8172 bytes_read=24557 bytes_retransmit=0 bytes_invalid=0 send_seq=676 receive_seq=676 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.29 cputime=14249.336 memavail=7241364 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635798.8: gcodein=0  mcu: mcu_awake=0.012 mcu_task_avg=0.000098 mcu_task_stddev=0.000086 bytes_write=8178 bytes_read=24657 bytes_retransmit=0 bytes_invalid=0 send_seq=677 receive_seq=677 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.29 cputime=14249.350 memavail=7241368 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635799.8: gcodein=0  mcu: mcu_awake=0.012 mcu_task_avg=0.000098 mcu_task_stddev=0.000086 bytes_write=8184 bytes_read=24771 bytes_retransmit=0 bytes_invalid=0 send_seq=678 receive_seq=678 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.27 cputime=14249.365 memavail=7241368 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.4 pwm=0.000
Stats 1635800.8: gcodein=0  mcu: mcu_awake=0.012 mcu_task_avg=0.000098 mcu_task_stddev=0.000086 bytes_write=8190 bytes_read=24885 bytes_retransmit=0 bytes_invalid=0 send_seq=679 receive_seq=679 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.27 cputime=14249.379 memavail=7241368 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635801.8: gcodein=0  mcu: mcu_awake=0.012 mcu_task_avg=0.000098 mcu_task_stddev=0.000086 bytes_write=8196 bytes_read=24985 bytes_retransmit=0 bytes_invalid=0 send_seq=680 receive_seq=680 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.27 cputime=14249.393 memavail=7241368 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635802.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=8202 bytes_read=25112 bytes_retransmit=0 bytes_invalid=0 send_seq=681 receive_seq=681 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.27 cputime=14249.408 memavail=7241368 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635803.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=8208 bytes_read=25226 bytes_retransmit=0 bytes_invalid=0 send_seq=682 receive_seq=682 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.3 pwm=0.000  sysload=0.27 cputime=14249.419 memavail=7251700 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635804.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=8214 bytes_read=25326 bytes_retransmit=0 bytes_invalid=0 send_seq=683 receive_seq=683 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.25 cputime=14249.427 memavail=7251700 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635805.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=8220 bytes_read=25440 bytes_retransmit=0 bytes_invalid=0 send_seq=684 receive_seq=684 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.3 pwm=0.000  sysload=0.25 cputime=14249.435 memavail=7251700 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635806.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=8226 bytes_read=25554 bytes_retransmit=0 bytes_invalid=0 send_seq=685 receive_seq=685 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.25 cputime=14249.443 memavail=7251700 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635807.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=8232 bytes_read=25654 bytes_retransmit=0 bytes_invalid=0 send_seq=686 receive_seq=686 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.25 cputime=14249.451 memavail=7251704 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635808.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=8238 bytes_read=25781 bytes_retransmit=0 bytes_invalid=0 send_seq=687 receive_seq=687 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.25 cputime=14249.463 memavail=7251704 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635809.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=8244 bytes_read=25895 bytes_retransmit=0 bytes_invalid=0 send_seq=688 receive_seq=688 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.22 cputime=14249.478 memavail=7251704 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635810.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=8250 bytes_read=25995 bytes_retransmit=0 bytes_invalid=0 send_seq=689 receive_seq=689 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.22 cputime=14249.492 memavail=7251704 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635811.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=8256 bytes_read=26109 bytes_retransmit=0 bytes_invalid=0 send_seq=690 receive_seq=690 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.22 cputime=14249.507 memavail=7251704 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635812.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=8262 bytes_read=26223 bytes_retransmit=0 bytes_invalid=0 send_seq=691 receive_seq=691 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.22 cputime=14249.521 memavail=7251704 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635813.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000069 bytes_write=8268 bytes_read=26336 bytes_retransmit=0 bytes_invalid=0 send_seq=692 receive_seq=692 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.22 cputime=14249.535 memavail=7251704 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635814.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000069 bytes_write=8274 bytes_read=26450 bytes_retransmit=0 bytes_invalid=0 send_seq=693 receive_seq=693 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.21 cputime=14249.548 memavail=7251200 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635815.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000069 bytes_write=8280 bytes_read=26564 bytes_retransmit=0 bytes_invalid=0 send_seq=694 receive_seq=694 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.21 cputime=14249.562 memavail=7251204 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635816.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000069 bytes_write=8286 bytes_read=26664 bytes_retransmit=0 bytes_invalid=0 send_seq=695 receive_seq=695 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.21 cputime=14249.575 memavail=7251204 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635817.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000069 bytes_write=8292 bytes_read=26778 bytes_retransmit=0 bytes_invalid=0 send_seq=696 receive_seq=696 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.21 cputime=14249.588 memavail=7251960 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635818.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000067 bytes_write=8298 bytes_read=26905 bytes_retransmit=0 bytes_invalid=0 send_seq=697 receive_seq=697 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.21 cputime=14249.602 memavail=7254488 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635819.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000067 bytes_write=8304 bytes_read=27005 bytes_retransmit=0 bytes_invalid=0 send_seq=698 receive_seq=698 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.19 cputime=14249.615 memavail=7254400 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635820.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000067 bytes_write=8310 bytes_read=27119 bytes_retransmit=0 bytes_invalid=0 send_seq=699 receive_seq=699 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.19 cputime=14249.627 memavail=7254400 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635821.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000067 bytes_write=8316 bytes_read=27233 bytes_retransmit=0 bytes_invalid=0 send_seq=700 receive_seq=700 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.19 cputime=14249.641 memavail=7254400 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635822.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000067 bytes_write=8322 bytes_read=27333 bytes_retransmit=0 bytes_invalid=0 send_seq=701 receive_seq=701 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.19 cputime=14249.654 memavail=7254400 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635823.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8328 bytes_read=27460 bytes_retransmit=0 bytes_invalid=0 send_seq=702 receive_seq=702 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.19 cputime=14249.668 memavail=7254400 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635824.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8334 bytes_read=27574 bytes_retransmit=0 bytes_invalid=0 send_seq=703 receive_seq=703 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.17 cputime=14249.682 memavail=7253896 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635825.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8340 bytes_read=27674 bytes_retransmit=0 bytes_invalid=0 send_seq=704 receive_seq=704 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.17 cputime=14249.694 memavail=7253900 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635826.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8346 bytes_read=27788 bytes_retransmit=0 bytes_invalid=0 send_seq=705 receive_seq=705 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.17 cputime=14249.708 memavail=7253900 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635827.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8352 bytes_read=27902 bytes_retransmit=0 bytes_invalid=0 send_seq=706 receive_seq=706 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.17 cputime=14249.722 memavail=7253396 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635828.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8358 bytes_read=28015 bytes_retransmit=0 bytes_invalid=0 send_seq=707 receive_seq=707 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.17 cputime=14249.735 memavail=7253396 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635829.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8364 bytes_read=28129 bytes_retransmit=0 bytes_invalid=0 send_seq=708 receive_seq=708 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.16 cputime=14249.749 memavail=7253396 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635830.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8370 bytes_read=28243 bytes_retransmit=0 bytes_invalid=0 send_seq=709 receive_seq=709 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.16 cputime=14249.762 memavail=7253396 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635831.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8376 bytes_read=28343 bytes_retransmit=0 bytes_invalid=0 send_seq=710 receive_seq=710 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.16 cputime=14249.776 memavail=7253396 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635832.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=8382 bytes_read=28457 bytes_retransmit=0 bytes_invalid=0 send_seq=711 receive_seq=711 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.16 cputime=14249.789 memavail=7253396 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635833.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000071 bytes_write=8388 bytes_read=28584 bytes_retransmit=0 bytes_invalid=0 send_seq=712 receive_seq=712 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.16 cputime=14249.803 memavail=7253396 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635834.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000071 bytes_write=8400 bytes_read=28700 bytes_retransmit=0 bytes_invalid=0 send_seq=714 receive_seq=714 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.15 cputime=14249.817 memavail=7253148 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635835.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000071 bytes_write=8406 bytes_read=28814 bytes_retransmit=0 bytes_invalid=0 send_seq=715 receive_seq=715 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.15 cputime=14249.830 memavail=7253148 print_time=144.326 buffer_time=0.000 print_stall=0 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635836.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000071 bytes_write=8562 bytes_read=28938 bytes_retransmit=0 bytes_invalid=0 send_seq=718 receive_seq=718 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.15 cputime=14249.850 memavail=7253148 print_time=190.983 buffer_time=5.100 print_stall=0 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635837.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000071 bytes_write=8568 bytes_read=29038 bytes_retransmit=0 bytes_invalid=0 send_seq=719 receive_seq=719 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.15 cputime=14249.864 memavail=7252140 print_time=190.983 buffer_time=4.099 print_stall=0 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635838.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000092 mcu_task_stddev=0.000094 bytes_write=8574 bytes_read=29166 bytes_retransmit=0 bytes_invalid=0 send_seq=720 receive_seq=720 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.15 cputime=14249.879 memavail=7252140 print_time=190.983 buffer_time=3.098 print_stall=1 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635839.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000092 mcu_task_stddev=0.000094 bytes_write=8580 bytes_read=29280 bytes_retransmit=0 bytes_invalid=0 send_seq=721 receive_seq=721 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.14 cputime=14249.894 memavail=7252140 print_time=190.983 buffer_time=2.097 print_stall=1 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635840.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000092 mcu_task_stddev=0.000094 bytes_write=8586 bytes_read=29380 bytes_retransmit=0 bytes_invalid=0 send_seq=722 receive_seq=722 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.14 cputime=14249.909 memavail=7252140 print_time=190.983 buffer_time=1.096 print_stall=1 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635841.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000092 mcu_task_stddev=0.000094 bytes_write=8867 bytes_read=29514 bytes_retransmit=0 bytes_invalid=0 send_seq=727 receive_seq=727 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.14 cputime=14249.930 memavail=7252140 print_time=201.033 buffer_time=10.146 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635842.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000092 mcu_task_stddev=0.000094 bytes_write=8873 bytes_read=29628 bytes_retransmit=0 bytes_invalid=0 send_seq=728 receive_seq=728 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.14 cputime=14249.944 memavail=7252140 print_time=201.033 buffer_time=9.145 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635843.8: gcodein=0  mcu: mcu_awake=0.010 mcu_task_avg=0.000105 mcu_task_stddev=0.000116 bytes_write=8879 bytes_read=29743 bytes_retransmit=0 bytes_invalid=0 send_seq=729 receive_seq=729 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.14 cputime=14249.959 memavail=7252140 print_time=201.033 buffer_time=8.145 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635844.8: gcodein=0  mcu: mcu_awake=0.010 mcu_task_avg=0.000105 mcu_task_stddev=0.000116 bytes_write=8885 bytes_read=29857 bytes_retransmit=0 bytes_invalid=0 send_seq=730 receive_seq=730 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.12 cputime=14249.974 memavail=7252584 print_time=201.033 buffer_time=7.144 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635845.8: gcodein=0  mcu: mcu_awake=0.010 mcu_task_avg=0.000105 mcu_task_stddev=0.000116 bytes_write=8891 bytes_read=29971 bytes_retransmit=0 bytes_invalid=0 send_seq=731 receive_seq=731 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.12 cputime=14249.988 memavail=7252644 print_time=201.033 buffer_time=6.143 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635846.8: gcodein=0  mcu: mcu_awake=0.010 mcu_task_avg=0.000105 mcu_task_stddev=0.000116 bytes_write=8897 bytes_read=30071 bytes_retransmit=0 bytes_invalid=0 send_seq=732 receive_seq=732 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999213 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.12 cputime=14250.001 memavail=7252644 print_time=201.033 buffer_time=5.142 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635847.8: gcodein=0  mcu: mcu_awake=0.010 mcu_task_avg=0.000105 mcu_task_stddev=0.000116 bytes_write=8903 bytes_read=30185 bytes_retransmit=0 bytes_invalid=0 send_seq=733 receive_seq=733 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.12 cputime=14250.015 memavail=7255428 print_time=201.033 buffer_time=4.141 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635848.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000087 mcu_task_stddev=0.000076 bytes_write=8909 bytes_read=30312 bytes_retransmit=0 bytes_invalid=0 send_seq=734 receive_seq=734 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.3 pwm=0.000  sysload=0.12 cputime=14250.029 memavail=7255428 print_time=201.033 buffer_time=3.140 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635849.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000087 mcu_task_stddev=0.000076 bytes_write=8915 bytes_read=30412 bytes_retransmit=0 bytes_invalid=0 send_seq=735 receive_seq=735 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.11 cputime=14250.043 memavail=7255428 print_time=201.033 buffer_time=2.139 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635850.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000087 mcu_task_stddev=0.000076 bytes_write=8921 bytes_read=30526 bytes_retransmit=0 bytes_invalid=0 send_seq=736 receive_seq=736 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.11 cputime=14250.057 memavail=7255428 print_time=201.033 buffer_time=1.139 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635851.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000087 mcu_task_stddev=0.000076 bytes_write=9127 bytes_read=30655 bytes_retransmit=0 bytes_invalid=0 send_seq=740 receive_seq=740 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.11 cputime=14250.076 memavail=7255176 print_time=206.083 buffer_time=5.189 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635852.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000087 mcu_task_stddev=0.000076 bytes_write=9133 bytes_read=30755 bytes_retransmit=0 bytes_invalid=0 send_seq=741 receive_seq=741 retransmit_seq=0 srtt=0.003 rttvar=0.002 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999212 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.11 cputime=14250.089 memavail=7255176 print_time=206.083 buffer_time=4.188 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635853.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000098 mcu_task_stddev=0.000101 bytes_write=9139 bytes_read=30883 bytes_retransmit=0 bytes_invalid=0 send_seq=742 receive_seq=742 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.11 cputime=14250.103 memavail=7255176 print_time=206.083 buffer_time=3.187 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635854.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000098 mcu_task_stddev=0.000101 bytes_write=9145 bytes_read=30997 bytes_retransmit=0 bytes_invalid=0 send_seq=743 receive_seq=743 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.18 cputime=14250.118 memavail=7254168 print_time=206.083 buffer_time=2.187 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635855.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000098 mcu_task_stddev=0.000101 bytes_write=9151 bytes_read=31097 bytes_retransmit=0 bytes_invalid=0 send_seq=744 receive_seq=744 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.18 cputime=14250.131 memavail=7254168 print_time=206.083 buffer_time=1.186 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635856.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000098 mcu_task_stddev=0.000101 bytes_write=9209 bytes_read=31216 bytes_retransmit=0 bytes_invalid=0 send_seq=746 receive_seq=746 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.18 cputime=14250.145 memavail=7254168 print_time=206.083 buffer_time=0.186 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635857.8: gcodein=0  mcu: mcu_awake=0.009 mcu_task_avg=0.000098 mcu_task_stddev=0.000101 bytes_write=9215 bytes_read=31330 bytes_retransmit=0 bytes_invalid=0 send_seq=747 receive_seq=747 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999211 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.18 cputime=14250.159 memavail=7253916 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635858.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000086 mcu_task_stddev=0.000076 bytes_write=9221 bytes_read=31443 bytes_retransmit=0 bytes_invalid=0 send_seq=748 receive_seq=748 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.18 cputime=14250.173 memavail=7253920 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635859.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000086 mcu_task_stddev=0.000076 bytes_write=9227 bytes_read=31557 bytes_retransmit=0 bytes_invalid=0 send_seq=749 receive_seq=749 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.25 cputime=14250.186 memavail=7253920 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635860.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000086 mcu_task_stddev=0.000076 bytes_write=9233 bytes_read=31671 bytes_retransmit=0 bytes_invalid=0 send_seq=750 receive_seq=750 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999210 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.25 cputime=14250.200 memavail=7253920 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635861.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000086 mcu_task_stddev=0.000076 bytes_write=9239 bytes_read=31771 bytes_retransmit=0 bytes_invalid=0 send_seq=751 receive_seq=751 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.25 cputime=14250.213 memavail=7253920 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635862.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000086 mcu_task_stddev=0.000076 bytes_write=9245 bytes_read=31899 bytes_retransmit=0 bytes_invalid=0 send_seq=752 receive_seq=752 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999208 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.25 cputime=14250.227 memavail=7253920 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635863.8: gcodein=0  mcu: mcu_awake=0.008 mcu_task_avg=0.000086 mcu_task_stddev=0.000076 bytes_write=9251 bytes_read=32012 bytes_retransmit=0 bytes_invalid=0 send_seq=753 receive_seq=753 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999208 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.25 cputime=14250.240 memavail=7253920 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635864.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9257 bytes_read=32112 bytes_retransmit=0 bytes_invalid=0 send_seq=754 receive_seq=754 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999208 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.31 cputime=14250.254 memavail=7253668 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635865.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9263 bytes_read=32240 bytes_retransmit=0 bytes_invalid=0 send_seq=755 receive_seq=755 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999209 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.31 cputime=14250.268 memavail=7253668 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635866.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9269 bytes_read=32340 bytes_retransmit=0 bytes_invalid=0 send_seq=756 receive_seq=756 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999208 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.31 cputime=14250.281 memavail=7253668 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635867.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9275 bytes_read=32440 bytes_retransmit=0 bytes_invalid=0 send_seq=757 receive_seq=757 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999207 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.31 cputime=14250.293 memavail=7253636 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635868.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000066 bytes_write=9281 bytes_read=32581 bytes_retransmit=0 bytes_invalid=0 send_seq=758 receive_seq=758 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999207 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.31 cputime=14250.307 memavail=7253636 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635869.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000066 bytes_write=9287 bytes_read=32681 bytes_retransmit=0 bytes_invalid=0 send_seq=759 receive_seq=759 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999206 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.29 cputime=14250.321 memavail=7253636 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635870.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000066 bytes_write=9293 bytes_read=32781 bytes_retransmit=0 bytes_invalid=0 send_seq=760 receive_seq=760 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999206 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.29 cputime=14250.334 memavail=7253636 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.0 pwm=0.000
Stats 1635871.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000066 bytes_write=9299 bytes_read=32909 bytes_retransmit=0 bytes_invalid=0 send_seq=761 receive_seq=761 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999206 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.29 cputime=14250.348 memavail=7253636 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635872.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000066 bytes_write=9305 bytes_read=33009 bytes_retransmit=0 bytes_invalid=0 send_seq=762 receive_seq=762 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999206 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.29 cputime=14250.361 memavail=7253636 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635873.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9311 bytes_read=33122 bytes_retransmit=0 bytes_invalid=0 send_seq=763 receive_seq=763 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999205 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.29 cputime=14250.374 memavail=7303188 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635874.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9317 bytes_read=33250 bytes_retransmit=0 bytes_invalid=0 send_seq=764 receive_seq=764 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999205 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.26 cputime=14250.382 memavail=7303160 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635875.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9323 bytes_read=33350 bytes_retransmit=0 bytes_invalid=0 send_seq=765 receive_seq=765 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999204 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.26 cputime=14250.390 memavail=7303160 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635876.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9329 bytes_read=33450 bytes_retransmit=0 bytes_invalid=0 send_seq=766 receive_seq=766 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999204 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.26 cputime=14250.398 memavail=7302300 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635877.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9335 bytes_read=33578 bytes_retransmit=0 bytes_invalid=0 send_seq=767 receive_seq=767 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999203 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.26 cputime=14250.408 memavail=7272652 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635878.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9341 bytes_read=33678 bytes_retransmit=0 bytes_invalid=0 send_seq=768 receive_seq=768 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999203 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.26 cputime=14250.419 memavail=7246380 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635879.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=9347 bytes_read=33791 bytes_retransmit=0 bytes_invalid=0 send_seq=769 receive_seq=769 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999202 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.80 cputime=14250.431 memavail=7206364 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.0 pwm=0.000
Stats 1635880.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=9353 bytes_read=33919 bytes_retransmit=0 bytes_invalid=0 send_seq=770 receive_seq=770 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999202 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.80 cputime=14250.442 memavail=7176928 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635881.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=9359 bytes_read=34019 bytes_retransmit=0 bytes_invalid=0 send_seq=771 receive_seq=771 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999202 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.80 cputime=14250.453 memavail=7140512 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635882.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=9365 bytes_read=34119 bytes_retransmit=0 bytes_invalid=0 send_seq=772 receive_seq=772 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999201 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.80 cputime=14250.462 memavail=7130568 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635883.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000068 bytes_write=9371 bytes_read=34247 bytes_retransmit=0 bytes_invalid=0 send_seq=773 receive_seq=773 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999201 heater_bed: target=0 temp=20.8 pwm=0.000  sysload=0.80 cputime=14250.474 memavail=7108240 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635884.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=9377 bytes_read=34360 bytes_retransmit=0 bytes_invalid=0 send_seq=774 receive_seq=774 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.82 cputime=14250.484 memavail=7100556 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635885.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=9383 bytes_read=34460 bytes_retransmit=0 bytes_invalid=0 send_seq=775 receive_seq=775 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.82 cputime=14250.492 memavail=7100304 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635886.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=9389 bytes_read=34588 bytes_retransmit=0 bytes_invalid=0 send_seq=776 receive_seq=776 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.82 cputime=14250.501 memavail=7098544 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635887.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=9395 bytes_read=34688 bytes_retransmit=0 bytes_invalid=0 send_seq=777 receive_seq=777 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.82 cputime=14250.509 memavail=7100304 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635888.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000081 mcu_task_stddev=0.000068 bytes_write=9401 bytes_read=34788 bytes_retransmit=0 bytes_invalid=0 send_seq=778 receive_seq=778 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.82 cputime=14250.517 memavail=7106924 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635889.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9407 bytes_read=34929 bytes_retransmit=0 bytes_invalid=0 send_seq=779 receive_seq=779 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.75 cputime=14250.531 memavail=7106924 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635890.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9413 bytes_read=35029 bytes_retransmit=0 bytes_invalid=0 send_seq=780 receive_seq=780 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.75 cputime=14250.544 memavail=7106924 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635891.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9419 bytes_read=35129 bytes_retransmit=0 bytes_invalid=0 send_seq=781 receive_seq=781 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.75 cputime=14250.557 memavail=7106928 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635892.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9425 bytes_read=35257 bytes_retransmit=0 bytes_invalid=0 send_seq=782 receive_seq=782 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.75 cputime=14250.571 memavail=7106112 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.4 pwm=0.000
Stats 1635893.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9431 bytes_read=35357 bytes_retransmit=0 bytes_invalid=0 send_seq=783 receive_seq=783 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.75 cputime=14250.584 memavail=7106424 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635894.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9437 bytes_read=35470 bytes_retransmit=0 bytes_invalid=0 send_seq=784 receive_seq=784 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.69 cputime=14250.593 memavail=7106572 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635895.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9449 bytes_read=35614 bytes_retransmit=0 bytes_invalid=0 send_seq=786 receive_seq=786 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.69 cputime=14250.601 memavail=7106676 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635896.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9455 bytes_read=35714 bytes_retransmit=0 bytes_invalid=0 send_seq=787 receive_seq=787 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.69 cputime=14250.609 memavail=7106676 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635897.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9461 bytes_read=35814 bytes_retransmit=0 bytes_invalid=0 send_seq=788 receive_seq=788 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.69 cputime=14250.617 memavail=7106200 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635898.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000079 mcu_task_stddev=0.000066 bytes_write=9467 bytes_read=35942 bytes_retransmit=0 bytes_invalid=0 send_seq=789 receive_seq=789 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.69 cputime=14250.625 memavail=7106200 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635899.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9473 bytes_read=36055 bytes_retransmit=0 bytes_invalid=0 send_seq=790 receive_seq=790 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.64 cputime=14250.638 memavail=7106360 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635900.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9479 bytes_read=36155 bytes_retransmit=0 bytes_invalid=0 send_seq=791 receive_seq=791 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.64 cputime=14250.652 memavail=7106452 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635901.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9485 bytes_read=36283 bytes_retransmit=0 bytes_invalid=0 send_seq=792 receive_seq=792 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.3 pwm=0.000  sysload=0.64 cputime=14250.664 memavail=7105024 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635902.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9491 bytes_read=36383 bytes_retransmit=0 bytes_invalid=0 send_seq=793 receive_seq=793 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.64 cputime=14250.673 memavail=7107272 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635903.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9497 bytes_read=36483 bytes_retransmit=0 bytes_invalid=0 send_seq=794 receive_seq=794 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.5 pwm=0.000  sysload=0.64 cputime=14250.681 memavail=7119368 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635904.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9503 bytes_read=36624 bytes_retransmit=0 bytes_invalid=0 send_seq=795 receive_seq=795 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999201 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.58 cputime=14250.689 memavail=7119368 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635905.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9509 bytes_read=36724 bytes_retransmit=0 bytes_invalid=0 send_seq=796 receive_seq=796 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.58 cputime=14250.697 memavail=7119368 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635906.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9515 bytes_read=36824 bytes_retransmit=0 bytes_invalid=0 send_seq=797 receive_seq=797 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.58 cputime=14250.707 memavail=7118864 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635907.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9521 bytes_read=36952 bytes_retransmit=0 bytes_invalid=0 send_seq=798 receive_seq=798 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999200 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.58 cputime=14250.716 memavail=7115364 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635908.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000066 bytes_write=9527 bytes_read=37052 bytes_retransmit=0 bytes_invalid=0 send_seq=799 receive_seq=799 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.58 cputime=14250.723 memavail=7115364 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635909.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=9533 bytes_read=37165 bytes_retransmit=0 bytes_invalid=0 send_seq=800 receive_seq=800 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999199 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.62 cputime=14250.731 memavail=7115364 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635910.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=9539 bytes_read=37293 bytes_retransmit=0 bytes_invalid=0 send_seq=801 receive_seq=801 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999198 heater_bed: target=0 temp=20.4 pwm=0.000  sysload=0.62 cputime=14250.739 memavail=7115364 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.1 pwm=0.000
Stats 1635911.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=9545 bytes_read=37393 bytes_retransmit=0 bytes_invalid=0 send_seq=802 receive_seq=802 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999198 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.62 cputime=14250.747 memavail=7115512 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635912.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=9551 bytes_read=37493 bytes_retransmit=0 bytes_invalid=0 send_seq=803 receive_seq=803 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999198 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.62 cputime=14250.759 memavail=7115620 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635913.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000078 mcu_task_stddev=0.000066 bytes_write=9557 bytes_read=37621 bytes_retransmit=0 bytes_invalid=0 send_seq=804 receive_seq=804 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999198 heater_bed: target=0 temp=20.7 pwm=0.000  sysload=0.62 cputime=14250.773 memavail=7115620 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635914.8: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=9563 bytes_read=37734 bytes_retransmit=0 bytes_invalid=0 send_seq=805 receive_seq=805 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999198 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.57 cputime=14250.785 memavail=7115768 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.3 pwm=0.000
Stats 1635915.9: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=9569 bytes_read=37840 bytes_retransmit=0 bytes_invalid=0 send_seq=806 receive_seq=806 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999198 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.57 cputime=14250.797 memavail=7115872 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
Stats 1635916.9: gcodein=0  mcu: mcu_awake=0.007 mcu_task_avg=0.000080 mcu_task_stddev=0.000068 bytes_write=9575 bytes_read=37946 bytes_retransmit=0 bytes_invalid=0 send_seq=807 receive_seq=807 retransmit_seq=0 srtt=0.003 rttvar=0.001 rto=0.025 ready_bytes=0 upcoming_bytes=0 freq=15999198 heater_bed: target=0 temp=20.6 pwm=0.000  sysload=0.57 cputime=14250.810 memavail=7115872 print_time=206.083 buffer_time=0.000 print_stall=2 extruder: target=0 temp=21.2 pwm=0.000
